
Commercial Work Bench


Assembly Instructions





Let the tabletop upside down


on a soft clotin to prevent scratches.

Insert one pipe into a comer support.









Remove the allen screws

and allen wrench.

Each corner support requires

Two allen screws.Wait until the

table is completely assembled

before securely tighening each allen screw.

After all four pipes have been

Attached,lower the adjustable

Table base and let each pipe

Into the base holes .

Each corner support requires

Two allen screws .Wait until the

table is completely assembled

before securely tightening each allen screw.

Insert four casters into the four foot tubes, all of which are universal wheels, two of which have brakes.

Turn the table over after each screw

is securely tightened .Two people

should be required to rotate the table.

